|  |  |  |  |
| --- | --- | --- | --- |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 getProvisData 17 parm: NULL, parm2 3 erro |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 getProvisData 17 parm: NULL, parm2 4 erro |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 getProvisData 17 parm: NULL, parm2 5 erro |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 cmSetCfgCodec: Endpt 0, Total 4 codecs, Packet Period: 20ms, GVAD Mode: TRANSPARENT, Fax Enabled: FALSE, CNG Mode: OFF, VBD codec: |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 cmSetCfgCodec: codec[0] = |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 cmSetCfgCodec: codec[1] = |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 cmSetCfgCodec: codec[2] = 7 |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 cmSetCfgCodec: codec[3] = |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 Don't need to start NAT keep a |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 cmFeatInit (summary) for line 0: fwd-busy=0, fwd-all=0, fwd-noans=0, c |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 Line 0 (98822): |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 Line 1 (): |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 REGISTER\_EVENT\_INTEREST for 0x10000280 succe |
| Apr 2 12:40:48 | daemon | warn | kernel: 12:40:48 SIP >>>>> Sent 520 bytes from 172.16.0.205:5060 to 0.0.0.0:0 > |
| Apr 2 12:40:48 | daemon | warn | kernel: REGISTER sip:172.16.0.1:5060 SIP/2 |
| Apr 2 12:40:48 | daemon | warn | kernel: Via: SIP/2.0/UDP 172.16.0.205;branch=z9hG4bK422b17e9d688a84 |
| Apr 2 12:40:48 | daemon | warn | kernel: Max-Forwards: |
| Apr 2 12:40:48 | daemon | warn | kernel: From: 98822 ;tag=8a2616eb |
| Apr 2 12:40:48 | daemon | warn | kernel: To: 98822<="" td=""> |
| Apr 2 12:40:48 | daemon | warn | kernel: Call-ID: 197a2e42ebb340 |
| Apr 2 12:40:48 | daemon | warn | kernel: CSeq: 1804289383 REGIST |
| Apr 2 12:40:48 | daemon | warn | kernel: Allow: INVITE, ACK, CANCEL, BYE, NOTIFY, REFER, OPTIONS, UPDATE, PRACK, IN |
| Apr 2 12:40:48 | daemon | warn | kernel: Contact: 98822 ;expires=36 |
| Apr 2 12:40:48 | daemon | warn | kernel: Privacy: no |
| Apr 2 12:40:48 | daemon | warn | kernel: Supported: pa |
| Apr 2 12:40:48 | daemon | warn | kernel: User-Agent: Brcm-Callctrl/v1.10.3 M5T SIP Stack/4.1.2 |
| Apr 2 12:40:48 | daemon | warn | kernel: Content-Length: |
| Apr 2 12:40:48 | daemon | warn | kernel |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:48 SIP <<<<< Recv 421 bytes from 172.16.0.1:5060 to 172.16.0.205:5060 < |
| Apr 2 12:40:49 | daemon | warn | kernel: SIP/2.0 401 Unauthoriz |
| Apr 2 12:40:49 | daemon | warn | kernel: Via: SIP/2.0/UDP 172.16.0.205;branch=z9hG4bK422b17e9d688a84 |
| Apr 2 12:40:49 | daemon | warn | kernel: From: 98822 ;tag=8a2616eb |
| Apr 2 12:40:49 | daemon | warn | kernel: To: "98822" ;tag=1642 |
| Apr 2 12:40:49 | daemon | warn | kernel: Call-ID: 197a2e42ebb340 |
| Apr 2 12:40:49 | daemon | warn | kernel: CSeq: 1804289383 REGIST |
| Apr 2 12:40:49 | daemon | warn | kernel: WWW-Authenticate: Digest realm="172.16.0.1", nonce="dea3ecee3a3d9e0ec5dc0401795f49d8", stale=TRUE, algorithm=M |
| Apr 2 12:40:49 | daemon | warn | kernel: User-Agent: smg\_pa\_sip smg\_pa\_sip-3.10.1. |
| Apr 2 12:40:49 | daemon | warn | kernel: Content-Length: |
| Apr 2 12:40:49 | daemon | warn | kernel |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 SIP >>>>> Sent 704 bytes from 172.16.0.205:5060 to 0.0.0.0:0 > |
| Apr 2 12:40:49 | daemon | warn | kernel: REGISTER sip:172.16.0.1:5060 SIP/2 |
| Apr 2 12:40:49 | daemon | warn | kernel: Via: SIP/2.0/UDP 172.16.0.205;branch=z9hG4bK96ec6927586e4f6 |
| Apr 2 12:40:49 | daemon | warn | kernel: Max-Forwards: |
| Apr 2 12:40:49 | daemon | warn | kernel: From: 98822 ;tag=8a2616eb |
| Apr 2 12:40:49 | daemon | warn | kernel: To: 98822<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: Call-ID: 197a2e42ebb340 |
| Apr 2 12:40:49 | daemon | warn | kernel: CSeq: 1804289384 REGIST |
| Apr 2 12:40:49 | daemon | warn | kernel: Allow: INVITE, ACK, CANCEL, BYE, NOTIFY, REFER, OPTIONS, UPDATE, PRACK, IN |
| Apr 2 12:40:49 | daemon | warn | kernel: Authorization: Digest username="98822",realm="172.16.0.1",nonce="dea3ecee3a3d9e0ec5dc0401795f49d8",uri="sip:172.16.0.1:5060",response="bb3b926da1cfa6b46f28dac75f48b370",algorithm=M |
| Apr 2 12:40:49 | daemon | warn | kernel: Contact: 98822 ;expires=36 |
| Apr 2 12:40:49 | daemon | warn | kernel: Privacy: no |
| Apr 2 12:40:49 | daemon | warn | kernel: Supported: pa |
| Apr 2 12:40:49 | daemon | warn | kernel: User-Agent: Brcm-Callctrl/v1.10.3 M5T SIP Stack/4.1.2 |
| Apr 2 12:40:49 | daemon | warn | kernel: Content-Length: |
| Apr 2 12:40:49 | daemon | warn | kernel |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmEventCallback: evt 5, cid -2147483648, sta -1, res 18, pkt 7edff518, |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 SIP <<<<< Recv 401 bytes from 172.16.0.1:5060 to 172.16.0.205:5060 < |
| Apr 2 12:40:49 | daemon | warn | kernel: SIP/2.0 200 |
| Apr 2 12:40:49 | daemon | warn | kernel: Via: SIP/2.0/UDP 172.16.0.205;branch=z9hG4bK96ec6927586e4f6 |
| Apr 2 12:40:49 | daemon | warn | kernel: From: 98822 ;tag=8a2616eb |
| Apr 2 12:40:49 | daemon | warn | kernel: To: "98822" ;tag=2839 |
| Apr 2 12:40:49 | daemon | warn | kernel: Call-ID: 197a2e42ebb340 |
| Apr 2 12:40:49 | daemon | warn | kernel: CSeq: 1804289384 REGIST |
| Apr 2 12:40:49 | daemon | warn | kernel: Contact: ;expires=36 |
| Apr 2 12:40:49 | daemon | warn | kernel: Date: Fri, 12 Apr 2019 09:14:54 G |
| Apr 2 12:40:49 | daemon | warn | kernel: User-Agent: smg\_pa\_sip smg\_pa\_sip-3.10.1. |
| Apr 2 12:40:49 | daemon | warn | kernel: Content-Length: |
| Apr 2 12:40:49 | daemon | warn | kernel |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 Voice start: voice status is Initializ |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 evt: 0x3005, op1: -2147483648, op2: 18, class: 0x |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmProcessCallEvent: cid 0x80000000, event 5 CCEVT\_STATUS, reason 18 CCRSN\_REG\_OK, packet 6a |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 Line 0 (98822): In Ser |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmEndpt: 0, cid -1: CMEVT\_INSERVICE in CMST\_ONHOOK endpt s |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 Setup ua-profile endpt 0 (cid 0) via '98822@172.16. |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 Subscribing endpt 0 (cid 0) to 'ua-profile;profile-type=user;vendor="Eltex";model="brcm-emta";version="1.10.1/1 |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 SIP >>>>> Sent 728 bytes from 172.16.0.205:5060 to 0.0.0.0:0 > |
| Apr 2 12:40:49 | daemon | warn | kernel: SUBSCRIBE sip:98822@172.16.0.1:5060 SIP/2 |
| Apr 2 12:40:49 | daemon | warn | kernel: Via: SIP/2.0/UDP 172.16.0.205;branch=z9hG4bK3c3f07703717da8 |
| Apr 2 12:40:49 | daemon | warn | kernel: Max-Forwards: |
| Apr 2 12:40:49 | daemon | warn | kernel: From: 98822 ;tag=45061d4c |
| Apr 2 12:40:49 | daemon | warn | kernel: To: 98822<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: Call-ID: c6e6bae5c82c45 |
| Apr 2 12:40:49 | daemon | warn | kernel: CSeq: 1374520142 SUBSCRI |
| Apr 2 12:40:49 | daemon | warn | kernel: Allow: INVITE, ACK, CANCEL, BYE, NOTIFY, REFER, OPTIONS, UPDATE, PRACK, IN |
| Apr 2 12:40:49 | daemon | warn | kernel: Contact: 98822<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: Event: ua-profile;profile-type=user;vendor="Eltex";model="brcm-emta";version="1.10.1/1. |
| Apr 2 12:40:49 | daemon | warn | kernel: Expires: 864 |
| Apr 2 12:40:49 | daemon | warn | kernel: P-Asserted-Identity: tel:P-Asserted-Identity, tel:P-Asserted-Identi |
| Apr 2 12:40:49 | daemon | warn | kernel: P-Preferred-Identity: 98822<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: Privacy: no |
| Apr 2 12:40:49 | daemon | warn | kernel: User-Agent: Brcm-Callctrl/v1.10.3 M5T SIP Stack/4.1.2 |
| Apr 2 12:40:49 | daemon | warn | kernel: Content-Length: |
| Apr 2 12:40:49 | daemon | warn | kernel |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmEventCallback: evt 5, cid 0, sta -1, res 45, pkt 7edff870, |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 SIP <<<<< Recv 458 bytes from 172.16.0.1:5060 to 172.16.0.205:5060 < |
| Apr 2 12:40:49 | daemon | warn | kernel: SIP/2.0 489 Bad Eve |
| Apr 2 12:40:49 | daemon | warn | kernel: Via: SIP/2.0/UDP 172.16.0.205;branch=z9hG4bK3c3f07703717da8 |
| Apr 2 12:40:49 | daemon | warn | kernel: From: 98822 ;tag=45061d4c |
| Apr 2 12:40:49 | daemon | warn | kernel: To: "98822"<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: Call-ID: c6e6bae5c82c45 |
| Apr 2 12:40:49 | daemon | warn | kernel: CSeq: 1374520142 SUBSCRI |
| Apr 2 12:40:49 | daemon | warn | kernel: Contact:<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: Error-Info:<="" td=""> |
| Apr 2 12:40:49 | daemon | warn | kernel: User-Agent: smg\_pa\_sip smg\_pa\_sip-3.10.1. |
| Apr 2 12:40:49 | daemon | warn | kernel: Content-Length: |
| Apr 2 12:40:49 | daemon | warn | kernel |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 evt: 0x3005, op1: 0, op2: 45, class: 0x |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmProcessCallEvent: cid 0x0, event 5 CCEVT\_STATUS, reason 45 CCRSN\_EVT\_SUBSCRIBE\_REJECT, packet 6a |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmCnxStateEngine: cid 0, ep 0: CMEVT\_SERVICE in CMST\_IDLE calls |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 cmProtCnxStateEngine: endpt=0, cid=0, cx->endpt=0, even |
| Apr 2 12:40:49 | daemon | warn | kernel: 12:40:49 Received response to CMS\_MSG\_REGISTER\_EVENT\_INTEREST fro |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 evt: 0x2006, op1: 1, op2: 0, class: 0x |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 endpt status pointer = 0x622f28, regStatus = 0, callStatus |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 evt: 0x2006, op1: 1, op2: 0, class: 0x |
| Apr 2 12:40:53 | daemon | warn | kernel: 12:40:53 endpt status pointer = 0x622f28, regStatus = 0, callStatus |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 evt: 0x2006, op1: 1, op2: 0, class: 0x |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 endpt status pointer = 0x622f28, regStatus = 0, callStatus |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 evt: 0x2006, op1: 1, op2: 0, class: 0x |
| Apr 2 12:41:13 | daemon | warn | kernel: 12:41:13 endpt status pointer = 0x622f28, regStatus = 0, callStatus |
| Apr 2 12:41:28 | daemon | alert | kernel: Intrusion -> IN=ppp0.1 OUT= MAC= SRC=81.22.45.249 DST=212.22.67.252 LEN=44 TOS=0x00 PREC=0x00 TTL=243 ID=12540 PROTO=TCP SPT=48965 DPT=3466 WINDOW=1024 RES=0x00 SYN URGP=0 MARK=0x8000 |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 evt: 0x2006, op1: 1, op2: 0, class: 0x |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 endpt status pointer = 0x622f28, regStatus = 0, callStatus |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 evt: 0x2006, op1: 0, op2: 0, class: 0x |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 endpt status pointer = 0x622f20, regStatus = 2, callStatus |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 processCmsMsg: CMS\_MSG\_VOICE\_CM\_ENDPT\_ST |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 evt: 0x2006, op1: 1, op2: 0, class: 0x |
| Apr 2 12:41:33 | daemon | warn | kernel: 12:41:33 endpt status pointer = 0x622f28, regStatus = 0, callStatus |